\href{https://saucelabs.com/u/ieee754}{\texttt{ }}\hypertarget{md_sfcode_node_modules_ieee754_README_autotoc_md12597}{}\doxysubsection{Read/write IEEE754 floating point numbers from/to a Buffer or array-\/like object.}\label{md_sfcode_node_modules_ieee754_README_autotoc_md12597}
\hypertarget{md_sfcode_node_modules_ieee754_README_autotoc_md12598}{}\doxysection{install}\label{md_sfcode_node_modules_ieee754_README_autotoc_md12598}

\begin{DoxyCode}{0}
\DoxyCodeLine{npm install ieee754 }

\end{DoxyCode}


\href{https://tidelift.com/subscription/pkg/npm-ieee754?utm_source=npm-ieee754&utm_medium=referral&utm_campaign=readme}{\texttt{ Get supported ieee754 with the Tidelift Subscription}}\hypertarget{md_sfcode_node_modules_ieee754_README_autotoc_md12599}{}\doxysection{methods}\label{md_sfcode_node_modules_ieee754_README_autotoc_md12599}
`var ieee754 = require(\textquotesingle{}ieee754')\`{}

The {\ttfamily ieee754} object has the following functions\+:


\begin{DoxyCode}{0}
\DoxyCodeLine{ieee754.read = function (buffer, offset, isLE, mLen, nBytes)}
\DoxyCodeLine{ieee754.write = function (buffer, value, offset, isLE, mLen, nBytes) }

\end{DoxyCode}


The arguments mean the following\+:


\begin{DoxyItemize}
\item buffer = the buffer
\item offset = offset into the buffer
\item value = value to set (only for {\ttfamily write})
\item is\+Le = is little endian?
\item m\+Len = mantissa length
\item n\+Bytes = number of bytes
\end{DoxyItemize}\hypertarget{md_sfcode_node_modules_ieee754_README_autotoc_md12600}{}\doxysection{what is ieee754?}\label{md_sfcode_node_modules_ieee754_README_autotoc_md12600}
The IEEE Standard for Floating-\/\+Point Arithmetic (IEEE 754) is a technical standard for floating-\/point computation. \href{http://en.wikipedia.org/wiki/IEEE_floating_point}{\texttt{ Read more}}.\hypertarget{md_sfcode_node_modules_ieee754_README_autotoc_md12601}{}\doxysection{license}\label{md_sfcode_node_modules_ieee754_README_autotoc_md12601}
BSD 3 Clause. Copyright (c) 2008, Fair Oaks Labs, Inc. 